Faults:

-sensor blocked => stop

-robot arm falls off

-robot moving

-light on top to make color detection easier, if the light is covered there is a disruption

-color error